OGRE Manual v1.4.7 ('Eihort'): Updating Index Buffers

[ < ] | [ Up ] | [ > ] |  |  |  |  |  |  |  | [Top] | [Contents] | [Index] | [ ? ]

### 5.7.2 Updating Index Buffers

Updating index buffers can only be done when you lock the buffer for writing; See section 5.4 Locking buffers for details. Locking returns a void pointer, which must be cast to the apropriate type; with index buffers this is either an unsigned short (for 16-bit indexes) or an unsigned long (for 32-bit indexes). For example:

    unsigned short* pIdx = static_cast<unsigned short*>(ibuf->lock(HardwareBuffer::HBL_DISCARD));

You can then write to the buffer using the usual pointer semantics, just remember to unlock the buffer when you're finished!

This document was generated by steve on March 5 2008 using texi2html